Directions for force direction change:

Step 1: Open the Force/Torque option at the dropdown menu on the External Loads Advisor and click the drop down for the part at the top right, find the component labelled pin B and click the drop down for that component.

Graphical user interface

Description automatically generated with medium confidence

Step 2: Click Selected direction to indicate that you will determine the direction of the force with respect to a certain component in the box marked with pink. Select the right plane in the dropdown menu for pin B for the selected direction, which will appear in the pink box as below.

Graphical user interface

Description automatically generated with low confidence

Step 3: For the face upon which the force is being applied in the blue box, select the face of your pin.

Graphical user interface

Description automatically generated

Step 4: Select a force value normal to the plane and change to your target value.

A screenshot of a computer

Description automatically generated with medium confidence